3 How to Access Each Device

> The table below shows how to access each device. Access with any procedure other than the ones shown below is prohibited.

Device | How to Read | Minimum Read Unit | How to Write | Minimum Write Unit
SRAM | "ReadSram" function "ReadSramFast" function | 1byte | "WriteSram" function "WriteSramFast" function | 1byte
FLASH | "ReadFlash" function | 1byte | "ProgramFlashSector" function | 4kbyte
EEPROM | "ReadEepromDword" function | 8byte | "ProgramEepromDword" function | 8byte
DACS | Direct read or "ReadDacs" (Either one is OK) | 2byte | "ProgramDacsSector" function "ProgramDacs_NE" function | Depends on the device and the function being used