SPARC targets

Contents|Index|Previous|Next
SPARC targets

The GNUPro Toolkit supports both the SPARC and the Fujitsu SPARClite families. For the compiler in particular, special configuration options allow you to use special software floating-point code for the SPARC MB86930 chip, as well as defaulting command-line options to use special Fujitsu SPARClite features.

For the Fujitsu SPARClite, the GNUPro Toolkit currently supports boards ex930, ex931, ex932, ex933, ex934, and ex936.

For documentation concerning the SPARC and SPARClite targets, see the following discussion.

- What to call the SPARC tools
- Compiling for SPARC targets

- Compiler options for SPARC
- Predefined preprocessor macros for SPARC
- Assembler options for SPARC

- Calling conventions for SPARC and SPARClite targets
- Debugging on SPARC and SPARClite targets
- Loading on specific atrgets for SPARC and SPARClite
- Further documentation for SPARClite

Top|Contents|Index|Previous|Next