What to call the tools for m68k

Contents|Index|Previous|Next
What to call the tools for m68k

Cross-development tools in the GNUPro Toolkit are normally installed with names that reflect the target machine, so that you can install more than one set of tools in the same binary directory. The target name, constructed with the ‘--target’ option to configure, is used as a prefix to the program name. For example, the compiler for the Motorola m68k (called simply gcc in native configurations) is called, depending on which configuration you have installed, by m68k-coff-gcc or m68k-aout-gcc.

The m68k-configured gdb is called by m68k-coff-gdb or m68k-aout-gdb.

For DOS-hosted toolchains, the tools are simply called by their standard names, such as gcc, gdb, etc.

Top|Contents|Index|Previous|Next