Assembler options for mips

Contents|Index|Previous|Next
Assembler options for MIPS

The following documentation discusses the assembler options for MIPS.

- Assembler options for listing output for MIPS
- Assembler listing-control directives for MIPS
- Assembler options for MIPS
- Assembler directives for debugging information for MIPS
- MIPS ECOFF object code
- Options for MIPS ECOFF object code
- Directives for MIPS ECOFF object code
- Registers used for integer arguments for MIPS
- Registers used for floating-point arguments for MIPS
- Calling conventions used for integer arguments for MIPS
- Calling conventions used for floating-point arguments for MIPS

To use the GNU assembler, as, to assemble gcc output, configure gcc with the switch, --with-gnu-as (in GNUPro Toolkit distributions) or with the option, -mgas. The assembler for MIPS architecture supports the MIPS R2000, R3000, and R4000 processors.

-mgas

Compile using as to assemble GCC output.

-Wa

If you invoke as through the GNU C compiler (version 2), you can use the -Wa option to pass arguments through to the assembler. One common use of this option is to exploit the assembler’s listing features. Assembler arguments that you specify with gcc -Wa must be separated from each other (and the -Wa) by commas.

-L

The additional assembler option -L preserves local labels, which may make the listing output more intelligible to humans. For example, in the following commandline, the assembler option, -ahl, requests a listing with interspersed high-level language and assembly language.

    $ h8300-hms-gcc -c -g -O -Wa,-alh,-L file.c

-L preserves local labels, while the compiler debugging option, -g, gives the assembler the necessary debugging information.

Assembler options for listing output for MIPS

Use the following options to enable listing output from the assembler (the letters after -a may be combined into one option, such as -aln):

-a

By itself, -a requests listings of high-level language source, assembly language, and symbols.

-ah

Requests a high-level language listing.

-al

Requests an output-program assembly listing.

-as

Requests a symbol table listing.

-ad

Omits debugging directives from the listing.

High-level listings require using a compiler debugging option like -g, and assembly listings (-al) also need to be requested.

Assembler listing-control directives for MIPS

Use the following listing-control assembler directives to control the appearance of the listing output (if you do not request listing output with one of the -a options, the following listing-control directives have no effect).

.list

Turn on listings from this point on.

.nolist

Turn off listings from this point on.

.psize linecount, columnwidth

Describe the page size for your output (the default is 60, 200). as generates form feeds after printing each group of linecount lines. To avoid these automatic form feeds, specify 0 as the linecount.

.eject

Skip to a new page (issue a form feed).

.title

Use heading as the title (this is the second line of the listing output, directly after the source file name and page number) when generating assembly listings.

.sbttl

Use subheading as the subtitle (this is the third line of the listing output, directly after the title line) when generating assembly listings.

-an

Turn off all forms processing.

Assembler options for MIPS

The MIPS configurations of as support three special options, and accept one other for command-line compatibility. See Command-line options in Using `as` in GNUPro Utilities for information on the command-line options available with all configurations of the GNU assembler.

-G num

This option sets the largest size of an object that will be referenced implicitly with the gp register. It is only accepted for targets that use ECOFF format. The default value is 8.

-EB
-EL

Any MIPS configuration of as can select big-endian or little-endian output at run time (unlike the other GNU development tools, which must be configured for one or the other). Use -EB to select big-endian output, and -EL for little-endian.

-nocpp

This option is ignored. It is accepted for command-line compatibility with other assemblers, which use it to turn off C style preprocessing. With the GNU assembler, there is no need for -nocpp, because the GNU assembler itself never runs the C preprocessor.

Assembler directives for debugging information for MIPS

MIPS ECOFF as supports several directives used for generating debugging information which are not supported by traditional MIPS assemblers:

        .def         .endef         .dim
        .file        .scl           .size
        .tag         .type          .val
        .stabd       .stabn         .stabs

The debugging information generated by the three .stab directives can only be read by gdb, not by traditional MIPS debuggers (this enhancement is required to fully support C++ debugging). These directives are primarily used by compilers, not assembly language programmers. See Assembler directives in Using `as` in GNUPro Utilities for full information on all GNU assembler directives.

MIPS ECOFF object code

The assembler supports some additional sections for a MIPS ECOFF target besides the usual .text, .data and .bss. The additional sections are:

.rdata

For readonly data

.sdata

For small data

.sbss

For small common objects. When assembling for ECOFF, the assembler uses the $gp ($28) register to form the address of a small object. Any object in the .sdata or .sbss section is considered small in this sense. Using small ECOFF objects requires linker support, and assumes that the $gp register has been correctly initialized (normally done automatically by the startup code).

Note:
MIPS ECOFF assembly code must not modify the $gp register.

Options for MIPS ECOFF object code

gcc -G

For external objects, or for objects in the .bss section, you can use the gcc -G option to control the size of objects addressed via $gp; the default value is 8, meaning that a reference to any object eight bytes or smaller will use $gp.

-G 0

Passing -G 0 to as prevents as from using the $gp register on the basis of object size (the assembler uses $gp for objects in .sdata or .sbss in any case).

Directives for MIPS ECOFF object code

.comm
.lcomm

The size of an object in the .bss section is set by the .comm or .lcomm directive that defines it.

.extern

The size of an external object may be set with the .extern directive. Use the following input, for example.

    .extern sym, 4

This directive declares that the object at sym is 4 bytes in length, while leaving sym otherwise undefined.

Registers used for integer arguments for MIPS
Arguments on MIPS architectures are not split, so that if a double word argument starts in R7, the entire word gets pushed onto the stack instead of being split between R7 and the stack.

If the first argument is an integer, the MIPS uses the following registers for all arguments.

The following calling convention for MIPS architectures depends on whether or not hardware floating-point is installed. Even if it is, the MIPS uses the registers for integer arguments whenever the first argument is an integer.

The MIPS uses the registers for floating-point arguments only for floating-point arguments and only if the first argument is a floating point.

The following calling convention for the MIPS also depends on whether you are using standard 32-bit mode or 64-bit mode; 32-bit mode only allows the MIPS to use even numbered registers, while 64-bit mode allows the MIPS to use both odd and even numbered registers.

- The MIPS passes the first four words of arguments in registers R4 through R7, which are also called registers A0 through A3.
- If the function return values are integers, they are stored in R2 and R3.

Note:
Functions compiled with different calling conventions cannot be run together without some care.

Registers used for floating-point arguments for MIPS

If the first argument is a floating-point, the MIPS uses the following registers for floating-point arguments.

- In 32-bit mode, the MIPS passes the first four words of arguments in registers F12 and F14.
- In 64-bit mode, the MIPS passes the first four words of arguments in registers F12 through F15.

If the function return value is a floating-point, it’s stored in F0.

Calling conventions used for integer arguments for MIPS
The following conventions apply to integer arguments.

R0 is hardwired to the value 0. R1, which is also called AT, is reserved as the assembler’s temporary register. R26 through R29 and R31 have reserved uses. Registers R2 through R15, R24, and R25 can be used for temporary values.

When a function is compiled with the default options, it must return with R16 through R23 and R30 unchanged.

Calling conventions used for floating-point arguments for MIPS
The following conventions apply to floating-point arguments. None of the registers has a reserved use.

- In 32-bit mode, F0 through F18 can be used for temporary values. When a function is compiled with the default options, it must return with F20 through F30 unchanged.
- In 64-bit mode, F0 through F19 can be used for temporary values. When a function is compiled with the default options, it must return with F20 through F31 unchanged.

Top|Contents|Index|Previous|Next