## Explanation of Work Area Structure "SoundArea"

With the structure, SoundArea, the following elements can be referenced. (Write is prohibited)
u8 reverb; // Reverb Value
u8 maxchn; // Simultaneously-produced Sounds
u8 masvol; // Master Volume
u8 freq; // Playback Frequency Number

// 1=5734Hz, 2=7884Hz,..., 12=42048Hz
The setting of these values is carried out with the previously described, SoundDriverMode(). When you want to reference the number of D/A conversion bits, directly read the AGB hardware register(REG_SOUNDBIAS bits 15-14).

[ | Back | Programmer's Manual Table of Contents | Using AGB Direct Sound Driver Table of Contents | Next | ]