MN10200 options

Contents|Index|Previous|Next
MN10200 options

The following ‘`-m`’ option is defined for the Matsushita MN10200 architecture.

  -mrelax

Indicate to the linker that it should perform a relaxation optimization pass to shorten branches, calls and absolute memory addresses. This option only has an effect when used on the command line for the final link step.

This option makes symbolic debugging impossible.